Controller RS485 relay via NetAssist

Demo :  https://youtu.be/olaK3FLNDgo

1 Connect the wires and power on

2 Set the IP address of the Ethernet port of the computer to "192.168.3.1"

3 Log in "192.168.3.7" on the browser

4 Switch the login interface to "ENGLISH"

5 Settings "Work mode":  -> TCP client/UDP Server ;

6 Settings "Local port":  -> 8887;

7 Settings "BaudRate":   ->9600;

8 Settings "MODBUS TCP to RTU":  -> Close;

9 Settings "MODBUS mode":  -> disable;

10 Click "submit",  Enter in the pop-up dialog: 123456

11 Open NetAssist


12 If "TCP client" cannot be used, "UDP Server" can be used

13 If you still cannot use it normally after setting the parameters, please restore the factory settings. and then reset the parameters